waits for mode3
enables mode 2 int
waits for int

on int jumps to 0x1000
some nops
reads stat
outputs value of stat&3

DMG-08 / CGB:
m2int_m2stat_1.gb should output 2
m2int_m2stat_2.gb should output 3
