waits for mode3
enables mode 2 int
waits for int

on int jumps to 0x1000
disables mode2 irq
nops til somewhere in or before next mode2
enables mode2 irq
reads IF
outputs value of IF&3

late_enable_1.gbc should output 2
late_enable_2.gbc should output 0
