waits for mode2
enables mode 0 int
waits for int

on int jumps to 0x1000
disables mode0 irq
nops til next mode0
writes 0x28 to ff41
sets IF to 0
writes 0x08 to ff41
reads IF
outputs value of IF&3

enable_twice_1.gbc should output 0
