waits until ly=3
sets lyc to 5
enables lyc int
waits for int

on int:
jumps to 0x1000
writes 0x20 to ff41
lots of nops
reads IF
outputs value of IF&3

enable_after_lycint_disable_1.gb should output 0
enable_after_lycint_disable_2.gb should output 2
