waits for mode3
enables mode 2 int
waits for int

on int jumps to 0x1000
enables mode0 irq
nops til mode0
reads IF
outputs value of IF&3

enable_after_m2_prior_1.gbc should output 2
enable_after_m2_prior_2.gbc should output 2
